Skip Navigation Links
Exit Print View
| Oracle Integrated Lights Out Manager (ILOM) 3.x ### Supplement for the Sun Blade 6000 Modular System

Search Scope:

- This Document
- Entire Library

### SNMP Traps

SNMP Traps are generated by the SNMP agents that are installed on the SNMP devices being managed by Oracle ILOM. Oracle ILOM receives the SNMP Traps and converts them into SNMP event messages that appear in the event log. For more information about the SNMP event messages that might be generated on your system, see the following table.

Note - For ILOM 3.1, replace `/CH` with `/SYSTEM`.

SNMP Event | SNMP Trap Sent | Sensor Name | Severity | Description
--- | --- | --- | --- | ---
Upper critical threshold exceeded | `sunHwTrapTempCritThresholdExceeded` | /CH/T_AMB /CH/PSx/T_AMB | Major | A temperature sensor has reported that its value has gone above an upper critical threshold setting or below a lower critical threshold setting. The sunHwTrapThresholdType object indicates whether the threshold was an upper or lower.
Upper critical threshold no longer exceeded | `sunHwTrapTempCritThresholdDeasserted` | /CH/T_AMB /CH/PSx/T_AMB | Informational | A temperature sensor has reported that its value has gone below an upper critical threshold setting or above a lower critical threshold setting. The sunHwTrapThresholdType object indicates whether the threshold was an upper or lower.
Upper fatal threshold exceeded | `sunHwTrapTempFatalThresholdExceeded` | /CH/T_AMB /CH/PSx/T_AMB | Critical | A temperature sensor has reported that its value has gone above an upper fatal threshold setting or below a lower fatal threshold setting. The sunHwTrapThresholdType object indicates whether the threshold was an upper or lower.
Upper fatal threshold no longer exceeded | `sunHwTrapTempFatalThresholdDeasserted` | /CH/T_AMB /CH/PSx/T_AMB | Informational | A temperature sensor has reported that its value has gone below an upper fatal threshold setting or above a lower fatal threshold setting. The sunHwTrapThresholdType object indicates whether the threshold was an upper or lower.
Assert | `sunHwTrapComponentError` | /CH/HOT /CH/BLx/ERR /CH/BLx/ESM/ERR /CH/NEMx/ERR /CH/PSx/V_3V3_ERR /CH/PSx/TEMP_WRN /CH/PSx/TEMP_ERR /CH/PSx/Sx/V_OUT_OK /CH/PSx/Sx/V_IN_ERR /CH/PSx/Sx/V_12V_ERR /CH/PSx/Sx/I_12V_ERR /CH/PSx/Sx/I_12V_WRN | Major | A sensor has detected an error. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type.
Deassert | `sunHwTrapComponentOk` | /CH/HOT /CH/BLx/ERR /CH/BLx/ESM/ERR /CH/NEMx/ERR /CH/PSx/V_3V3_ERR /CH/PSx/TEMP_WRN /CH/PSx/TEMP_ERR /CH/PSx/Sx/V_OUT_OK /CH/PSx/Sx/V_IN_ERR /CH/PSx/Sx/V_12V_ERR /CH/PSx/Sx/I_12V_ERR /CH/PSx/Sx/I_12V_WRN | Informational | A sensor has returned to its normal state. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type.
Lower fatal threshold exceeded | `sunHwTrapFanSpeedFatalThresholdExceeded` | /CH/PSx/FANx/TACH | Critical | A fan speed sensor has reported that its value has gone above an upper fatal threshold setting or below a lower fatal threshold setting. The sunHwTrapThresholdType object indicates whether the threshold was an upper or lower.
Lower fatal threshold no longer exceeded | `sunHwTrapFanSpeedFatalThresholdDeasserted` | /CH/PSx/FANx/TACH | Informational | A fan speed sensor has reported that its value has gone below an upper fatal threshold setting or above a lower fatal threshold setting. The sunHwTrapThresholdType object indicates whether the threshold was an upper or lower.
Remove | `sunHwTrapFruRemoved` | /CH/BLx /CH/NEMx /CH/PSx | Informational | A field replaceable unit has been removed from the system.
Insert | `sunHwTrapFruInserted` | /CH/BLx /CH/NEMx /CH/PSx | Informational | A field replaceable unit has been inserted into the system.
Install error | `sunHwTrapComponentError` | /CH/BLx/STATE /CH/NEMx/STATE | Major | A sensor has detected an error. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type.
Assert | `sunHwTrapFanError` | /CH/FMx/ERR /CH/PSx/FAN_ERR | Major | A fan sensor has detected an error.
Deassert | `sunHwTrapFanOk` | /CH/FMx/ERR /CH/PSx/FAN_ERR | Informational | A fan sensor has returned to its normal state.
event fault.chassis.device.fail | `sunHwTrapComponentFault` | /CH/FM /CH/BL | Major | A component is suspected of causing a fault. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type.
event fault.chassis.device.fail cleared | `sunHwTrapComponentFaultCleared` | /CH/FM /CH/BL | Informational | A component fault has been cleared. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type.
event fault.chassis.env.power.loss | `sunHwTrapPowerSupplyFault` | /CH/PS | Major | A power supply component is suspected of causing a fault.
event fault.chassis.env.power.loss cleared | `sunHwTrapPowerSupplyFaultCleared` | /CH/PS | Informational | A power supply component fault has been cleared.
event fault.chassis.power.undervoltage | `sunHwTrapPowerSupplyFault` | /CH/PS | Major | A power supply component is suspected of causing a fault.
event fault.chassis.power.undervoltage cleared | `sunHwTrapPowerSupplyFaultCleared` | /CH/PS | Informational | A power supply component fault has been cleared.
event fault.chassis.power.overcurrent | `sunHwTrapPowerSupplyFault` | /CH/PS | Major | A power supply component is suspected of causing a fault.
event fault.chassis.power.overcurrent cleared | `sunHwTrapPowerSupplyFaultCleared` | /CH/PS | Informational | A power supply component fault has been cleared.
event fault.chassis.power.overtemperature | `sunHwTrapPowerSupplyFault` | /CH/PS | Major | A power supply component is suspected of causing a fault.
event fault.chassis.power.overtemperature cleared | `sunHwTrapPowerSupplyFaultCleared` | /CH/PS | Informational | A power supply component fault has been cleared.
event fault.chassis.device.fan.fail | `sunHwTrapPowerSupplyFault` | /CH/PS | Major | A power supply component is suspected of causing a fault.
event fault.chassis.device.fan.fail cleared | `sunHwTrapPowerSupplyFaultCleared` | /CH/PS | Informational | A power supply component fault has been cleared.
event fault.chassis.device.missing | `sunHwTrapComponentFault` | /CH | Major | A component is suspected of causing a fault. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type.
event fault.chassis.device.missing cleared | `sunHwTrapComponentFaultCleared` | /CH | Informational | A component fault has been cleared. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type.
event fault.chassis.env.power.loss | `sunHwTrapComponentFault` | /CH/PS/S | Major | A component is suspected of causing a fault. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type.
event fault.chassis.env.power.loss cleared | `sunHwTrapComponentFaultCleared` | /CH/PS/S | Informational | A component fault has been cleared. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type.
event fault.chassis.device.psu.fail | `sunHwTrapPowerSupplyFault` | /CH/PS | Major | A power supply component is suspected of causing a fault.
event fault.chassis.device.psu.fail cleared | `sunHwTrapPowerSupplyFaultCleared` | /CH/PS | Informational | A power supply component fault has been cleared.
event fault.chassis.device.psu.fail | `sunHwTrapComponentFault` | /CH/PS/S | Major | A component is suspected of causing a fault. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type.
event fault.chassis.device.psu.fail cleared | `sunHwTrapComponentFaultCleared` | /CH/PS/S | Informational | A component fault has been cleared. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type.
event fault.chassis.power.overcurrent | `sunHwTrapComponentFault` | /CH/PS/S | Major | A component is suspected of causing a fault. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type.
event fault.chassis.power.overcurrent cleared | `sunHwTrapComponentFaultCleared` | /CH/PS/S | Informational | A component fault has been cleared. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type.
event fault.chassis.device.fan.fail | `sunHwTrapComponentFault` | /CH/PS/FAN | Major | A component is suspected of causing a fault. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type.
event fault.chassis.device.fan.fail cleared | `sunHwTrapComponentFaultCleared` | /CH/PS/FAN | Informational | A component fault has been cleared. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type.
event fault.chassis.env.temp.over-warn | `sunHwTrapComponentFault` | /CH | Major | A component is suspected of causing a fault. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type.
event fault.chassis.env.temp.over-warn cleared | `sunHwTrapComponentFaultCleared` | /CH | Informational | A component fault has been cleared. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type.
event fault.chassis.env.temp.over-fail | `sunHwTrapComponentFault` | /CH | Major | A component is suspected of causing a fault. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type.
event fault.chassis.env.temp.over-fail cleared | `sunHwTrapComponentFaultCleared` | /CH | Informational | A component fault has been cleared. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type.
event fault.chassis.device.fail | `sunHwTrapIOFault` | /CH/NEM | Major | A component in the IO subsystem is suspected of causing a fault.
event fault.chassis.device.fail cleared | `sunHwTrapIOFaultCleared` | /CH/NEM | Informational | An IO subsystem component fault has been cleared.
event fault.fruid.corrupt | `sunHwTrapIOFault` | /CH/NEM | Major | A component in the IO subsystem is suspected of causing a fault.
event fault.fruid.corrupt cleared | `sunHwTrapIOFaultCleared` | /CH/NEM | Informational | An IO subsystem component fault has been cleared.
event fault.chassis.device.population-invalid | `sunHwTrapComponentFault` | /CH | Major | A component is suspected of causing a fault. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type.
event fault.chassis.device.population-invalid cleared | `sunHwTrapComponentFaultCleared` | /CH | Informational | A component fault has been cleared. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type.
event fault.chassis.device.sas-expander.fail | `sunHwTrapComponentFault` | /CH/BL | Major | A component is suspected of causing a fault. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type.
event fault.chassis.device.sas-expander.fail cleared | `sunHwTrapComponentFaultCleared` | /CH/BL | Informational | A component fault has been cleared. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type.
event fault.chassis.device.sas-expander.fail | `sunHwTrapIOFault` | /CH/NEM | Major | A component in the IO subsystem is suspected of causing a fault.
event fault.chassis.device.sas-expander.fail cleared | `sunHwTrapIOFaultCleared` | /CH/NEM | Informational | An IO subsystem component fault has been cleared.
event fault.fruid.corrupt | `sunHwTrapComponentFault` | /CH/BL | Major | A component is suspected of causing a fault. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type.
event fault.fruid.corrupt cleared | `sunHwTrapComponentFaultCleared` | /CH/BL | Informational | A component fault has been cleared. This generic ’component’ trap is generated when the SNMP agent does not recognize the component type
Multiple events1 | `sunHwTrapComponentOk` | /CH/BLx/STATE /CH/NEMx/STATE | Informational | A sensor has returned to its normal state. This generic ‘component’ trap is generated when the SNMP agent does not recognize the component type.

1Events include: Transition to Running, Transition to In Test, Transition to Power Off, Transition to On Line, Transition to Off Line, Transition to Off Duty, Transition to Degraded, Transition to Power Save

Copyright © , 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |