Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Overview

Search Scope:

- This Document
- Entire Library

### Chassis

The following topics describe the Sun Blade 6000 modular system chassis.

- Chassis Description

- Identifying Chassis Models

##### Chassis Description

The chassis is the physical enclosure that contains the system components. It is designed for rackmounting and can be mounted into 19-inch EIA-310D cabinets with a depth of 35.4 to 39.4 inches (90.0 to 100.1 cm). The chassis can accommodate corresponding front-to-back, rail-to-rail spacing of 26.77 inches (68.0 cm) to 34.25 inches (87.0 cm).

| Caution - The chassis requires clear airflow from front to back. If doors are installed on the rack, they must be properly vented. Also, all blade slots must be occupied by either a blade or a blank filler panel.

Additional chassis specifications are available in the Sun Blade 6000 Modular System Site Planning Guide.

##### Identifying Chassis Models

The A90-D chassis contains the following components that are updated from the A90-A and B chassis models: CMM, midplane, rear fans, and power supplies.

The 7105379 chassis and associated components are functionally equivalent to A90-D and meet the requirements for EU Directive 2011/65/EU. The 7105379 chassis contains an updated CMM and midplane assembly.

Make sure that you know which chassis that you have. Some replaceable components are not interchangeable between the chassis.

Refer to Sun Blade 6000 Modular System Service Manual for additional methods for identifying which model of the chassis that you have.

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |