Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

#### Power Supply LEDs

The chassis contains two power supply modules (P0 and P1) and each power supply module contains two sides (S0 and S1). Each power supply module also contains a fan. The following illustration and table describes the power supply LEDs and their behavior.

No. | LED Description | Normal | Overcurrent | AC0 Failed | AC1 Failed | Front Fan Failed
--- | --- | --- | --- | --- | --- | ---
1 | Service Action Required | Off | On | Off | Off | Off
2 | DC (green) | On | Off | Off | Off | Off
3 | AC-1 (green) | On | On | On | Off | On
4 | AC-0 (green) | On | On | Off | On | On
5 | Fan Service (amber) | Off | Off | Off | Off | On

##### Related Information

- Chassis and CMM LEDs

- Rear Fan LEDs

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |