Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Site Planning Guide

Search Scope:

- This Document
- Entire Library

### Thermal Design Specifications

The thermal design specifications of the system are shown in the following table.

Parameter | Specification
--- | ---
Maximum possible system volumetric airflow | 1012 CFM
Maximum possible heat dissipation/HVAC load | 21,325 BTU/hr
Maximum possible temperature rise through chassis | 18.5o C (33o F)

Copyright © 2008, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |