Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

## Install a Server or Storage Module

1. If a filler panel is in the slot, remove the filler panel.
2. Rotate the lower ejector lever on the filler panel downward, and pull the filler panel out of the chassis.

   Note - Do not discard the filler panel. You must reinstall the filler panel if the server or storage module ever needs to be serviced or removed again.

3. Align the server or storage module with the vacant slot.
4. Ensure the following:

   - The server or storage module indicator LEDs on the front panel are facing toward you.

   - The server or storage module ejector levers are fully opened.

   - The server or storage module ejectors are on the right side of the module.

5. Slide the server or storage module into the vacant server module chassis slot.

   As the ejectors make contact with the chassis, the bottom lever begins to rise, and the top lever begins to lower.

6. Simultaneously close the ejector levers at the top and bottom of the server or storage module (lower the top ejector and raise the bottom ejector) until the levers clamp in place against the front of the server or storage module.

   As the ejector levers are closed, the server or storage module moves back to engage with the chassis.

7. Verify that the server or storage module is powered on and operational.

   After you insert a server or storage module into a powered-on system, the internal SP is brought online automatically, and the server or storage module is powered on by default.

##### Related Information

- Remove a Server or Storage Module

- Server module documentation at: http://www.oracle.com/technetwork/documentation/oracle-blade-sys-190001.html

- Monitoring Faults

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |