Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

## Depopulate the Chassis

Follow these steps if you plan to remove the chassis from the rack without a mechanical lift. If you plan to use a mechanical lift, go to Remove the Chassis From the Rack.

Depopulating the chassis makes the chassis much lighter, but manual chassis removal requires four people.

1. Label and record the locations of the all components in the modular system.

   Performing this step ensures that each component can be returned to its original location.

2. Use an antistatic wrist strap.

   Attach this wrist strap to your wrist and ground the other end of strap to the system chassis.

3. Remove the following components from the chassis:

   - Power supply unit – See: Remove a Power Supply.

   - Server/storage module – See Remove a Server or Storage Module.

   - PCIe EM – See Remove a PCIe EM.

   - NEM – See Remove a NEM.

   - Rear fan module – See Remove a Rear Fan Module.

   - CMM – See Remove the CMM.

   - Filler panel – See Remove a Server or Storage Module.

##### Related Information

- Remove the Chassis From the Rack

- Repopulate the Chassis

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |