Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Site Planning Guide

Search Scope:

- This Document
- Entire Library

### Acoustic Noise Emissions

Declared noise emissions are in accordance with ISO 9295/9296 standards.

Data center personnel should take necessary precautions to reduce exposure to the high noise levels. Acoustic noise emission levels are shown in the following table.

Function | Specification
--- | ---
Operating/idling acoustic noise (LwAd, 1B=10 dB) | 8.6 B at or below 25o C, 9.2 B at maximum ambient

Copyright © 2008, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |