Skip Navigation Links
Exit Print View
| Oracle Integrated Lights Out Manager (ILOM) 3.x ### Supplement for the Sun Blade 6000 Modular System

Search Scope:

- This Document
- Entire Library

### PET Event Messages

PET events are generated by systems with ASF or an IPMI baseboard management controller. The PET events provide advance warning of possible system failures. For more information about the PET event messages that might occur on your system, see the following table.

Note - For ILOM 3.1, replace `/CH` with `/SYSTEM`.

PET Event | PET Sent | Sensor Name | Severity | Description
--- | --- | --- | --- | ---
Temperature Upper critical threshold has been exceeded | `petTrapTemperatureUpperNonCriticalGoingHigh` | /CH/T_AMB /CH/PSx/T_AMB | Major | Temperature has increased above upper critical threshold.
Temperature Upper critical threshold no longer exceeded | `petTrapTemperatureUpperNonCriticalGoingLowDeassert` | /CH/T_AMB /CH/PSx/T_AMB | Warning | Temperature has decreased below upper critical threshold.
Temperature Lower fatal threshold has been exceeded | `petTrapTemperatureUpperNonRecoverableGoingHigh` | /CH/T_AMB /CH/PSx/T_AMB | Critical | Temperature has increased above upper non-recoverable threshold.
Temperature Lower fatal threshold no longer exceeded | `petTrapTemperatureUpperNonRecoverableGoingLowDeassert` | /CH/T_AMB /CH/PSx/T_AMB | Major | Temperature has decreased below upper non-recoverable threshold.
Temperature sensor ASSERT | `petTrapTemperatureStateAssertedAssert` | /CH/HOT | Critical | Temperature event occured. Possible cause: CPU is too hot.
Temperature sensor DEASSERT | `petTrapTemperatureStateDeassertedAssert` | /CH/HOT | Informational | Temperature event occured.
Entity Presence Insert | `petTrapEntityPresenceDeviceInsertedAssert` | /CH/BLx/PRSNT /CH/BLx/HDDx/PRSNT /CH/BLx/FMODx/PRSNT /CH/BLx/ESM/PRSNT /CH/NEMx/PRSNT /CH/PSx/PRSNT | Informational | A device is present or has been inserted.
Entity Presence Remove | `petTrapEntityPresenceDeviceRemovedAssert` | /CH/BLx/PRSNT /CH/BLx/HDDx/PRSNT /CH/BLx/FMODx/PRSNT /CH/BLx/ESM/PRSNT /CH/NEMx/PRSNT /CH/PSx/PRSNT | Informational | A device is absent or has been removed.
Module Transition to Running assert | `petTrapModuleBoardTransitionToRunningAssert` | /CH/BLx/STATE /CH/NEMx/STATE | Informational | A device has transitioned to the normal running state. For a blade, this indicates that the host has powered on.
Module Transition to In Test assert | `petTrapModuleBoardTransitionToInTestAssert` | /CH/BLx/STATE /CH/NEMx/STATE | Informational | A device is in a transitional state. (Used only for NEMs.)
Module Transition to Power Off assert | `petTrapModuleBoardTransitionToPowerOffAssert` | /CH/BLx/STATE /CH/NEMx/STATE | Informational | A device has powered off.
Module Transition to On Line assert | `petTrapModuleBoardTransitionToOnLineAssert` | /CH/BLx/STATE /CH/NEMx/STATE | Informational | A device is online and ready to enter the running state. (Used only for NEMs.)
Module Transition to Off Line assert | `petTrapModuleBoardTransitionToOffLineAssert` | /CH/BLx/STATE /CH/NEMx/STATE | Informational | Unused.
Module Transition to Off Duty assert | `petTrapModuleBoardTransitionToOffDutyAssert` | /CH/BLx/STATE /CH/NEMx/STATE | Informational | A device is no longer in use and is ready to be removed.
Module Transition to Degraded assert | `petTrapModuleBoardTransitionToDegradedAssert` | /CH/BLx/STATE /CH/NEMx/STATE | Informational | A device has entered a state of degraded operation, for example, due to a hardware fault, or an over-temperature condition that caused the device to shut itself down.
Module Transition to Power Save assert | `petTrapModuleBoardTransitionToPowerSaveAssert` | /CH/BLx/STATE /CH/NEMx/STATE | Informational | Unused.
Module Install Error assert | `petTrapModuleBoardInstallErrorAssert` | /CH/BLx/STATE /CH/NEMx/STATE | Informational | Unused.
OEM Reserved reporting Predictive Failure | `petTrapOEMPredictiveFailureAsserted 12583937` | /CH/BLx/ERR /CH/BLx/ESM/ERR /CH/NEMx/ERR | Major | OEM predictive failure asserted.
OEM Reserved Return to normal | `petTrapOEMPredictiveFailureDeasserted` | /CH/BLx/ERR /CH/BLx/ESM/ERR /CH/NEMx/ERR | Informational | OEM predictive failure deasserted.
Fan reporting Predictive Failure | `petTrapFanPredictiveFailureAsserted` | /CH/FMx/ERR /CH/PSx/FAN_ERR | Major | Fan predictive failure is detected.
Fan Return to normal | `petTrapFanPredictiveFailureDeasserted` | /CH/FMx/ERR /CH/PSx/FAN_ERR | Informational | Fan predictive failure state is cleared.
Voltage reporting Predictive Failure | `petTrapVoltagePredictiveFailureAssertedAssert` | /CH/PSx/V_3V3_ERR /CH/PSx/Sx/V_IN_ERR /CH/PSx/Sx/V_12V_ERR | Major | Voltagepredictive failure is detected.
Voltage Return to normal | `petTrapVoltagePredictiveFailureDeassertedAssert` | /CH/PSx/V_3V3_ERR /CH/PSx/Sx/V_IN_ERR /CH/PSx/Sx/V_12V_ERR | Informational | Predictive failure state due to voltage event has been cleared.
Temperature reporting Predictive Failure | `petTrapTemperaturePredictiveFailureAsserted` | /CH/PSx/TEMP_WRN /CH/PSx/TEMP_ERR | Major | System is reporting a predictive failure as a result of high temperature.
Temperature Return to normal | `petTrapTemperaturePredictiveFailureDeasserted` | /CH/PSx/TEMP_WRN /CH/PSx/TEMP_ERR | Informational | Predictive failure state due to high temperature has been cleared.
Fan Lower fatal threshold has been exceeded | `petTrapFanLowerNonRecoverableGoingLow` | /CH/PSx/FANx/TACH | Critical | Fan speed has decreased below lower non-recoverable threshold. Fan failed or removed.
Fan Lower fatal threshold no longer exceeded | `petTrapFanLowerNonRecoverableGoingHighDeassert` | /CH/PSx/FANx/TACH | Major | Fan speed has increased above lower non-recoverable threshold.
Voltage sensor ASSERT | `petTrapVoltageStateAssertedAssert` | /CH/PSx/Sx/V_OUT_OK | Informational | Voltage event has occurred.
Voltage sensor DEASSERT | `petTrapVoltageStateDeassertedAssert` | /CH/PSx/Sx/V_OUT_OK | Informational | Voltage event has occurred.
Current reporting Predictive Failure | `petTrapCurrentPredictiveFailureAsserted` | /CH/PSx/Sx/I_12V_ERR /CH/PSx/Sx/I_12V_WRN | Major | Predictive failure due to electric current conditions.
Current Return to normal | `petTrapCurrentPredictiveFailureDeasserted` | /CH/PSx/Sx/I_12V_ERR /CH/PSx/Sx/I_12V_WRN | Informational | Predictive failure caused by electric current conditions.

Copyright © , 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |