Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Site Planning Guide

Search Scope:

- This Document
- Entire Library

#### Electrical Requirements

The data center must meet the following electrical requirements for installation of a Sun Blade 6000 system:

- Four 200–240 VAC, 16A/20A branch circuits, one for each of the AC inlets on the system, are required.

  Each AC inlet requires a separate power cord; therefore, four power cords are required. The power cord must be rated at 16A or 20A, depending on the site location.

- If you are using an Oracle MPS in the cabinet, refer to the documentation supplied with the cabinet for the MPS power requirements.

- If you are not using an MPS, you must supply a branch circuit with a connector that meets the requirements of your system.

Copyright © 2008, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |