Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

## Remove a Server or Storage Module

1. Initiate an orderly shutdown of the operating system.

   For instructions, refer to the documentation for your server module.

2. Power down the server or storage module to standby power.
3. Press the levers on the ejectors at the top and bottom of the server or storage module.
4. Swing out both ejector levers simultaneously (raise the top ejector and lower the bottom ejector).
5. Use the ejector levers to start pulling the server module out of its slot in the chassis.

   | Caution - Do not use the ejector levers to carry the server or storage module. The ejector levers should be used only to unseat the server or storage module from the chassis. The levers are not designed to support the weight of the server or storage module.

6. Finish pulling the server or storage module out of the chassis, supporting the weight of the server or storage module from the bottom.
7. Install a filler panel into the server or storage module slot if the server or storage module will be out of the chassis for longer than one minute.

##### Related Information

- Install a Server or Storage Module

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |