Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Overview

Search Scope:

- This Document
- Entire Library

#### Guidelines for Updating Firmware

Specific instructions for updating chassis and component firmware are available in the Sun Blade 6000 Modular System Firmware Update Guide.

The following are general guidelines for updating chassis firmware:

- You can upgrade Sun Blade 6000 chassis, server module, and NEM firmware independently.

- You should always update server module firmware before updating the CMM firmware.

- If a NEM firmware update is required, you should install it after updating CMM firmware.

| Caution - Some firmware upgrade procedures remove a component from service. For example, server module ILOM upgrade procedures might shut down the server to perform BIOS upgrades. NEM and storage module firmware upgrades (or hot-swapping) might interrupt I/O connectivity to multiple blades.

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |