Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Site Planning Guide

Search Scope:

- This Document
- Entire Library

### AC Power Requirements

The AC power requirements of the system are shown in the following table.

Power Type | Function | Specification
--- | --- | ---
AC Power | Input power | 1+1 PSU rating, 6272 W or 6400 VA each power supply module
| Voltage | 200 to 240 VAC
| Frequency | 50 to 60 Hz
| Current | 16A per output, total four AC inputs (two per power supply module).
| Number of AC inputs | 4
| AC input connection | Americas Domestic – NEMA L6-20P to IEC320-C19M (4m, Oracle PN X5044A-Z) International – IEC309, 250 V, 16 A, 3 Pin to IEC320-C19 (4m, Oracle PN X5045A-Z) Installed in rack with modular power system – IEC320-C319 to IEC320-C20 (1.5m, Oracle PN X5046A-Z; (2.0m, X5047A-Z)
DC Power | Output power | 1+1 PSU rating, 5740 W each power supply module

Copyright © 2008, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |