Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

### Identifying Component Types and Service Classifications

All components in the modular system are removable and serviceable by a single person. There are two types of server module components:

- CRU – Customer-replaceable units can be removed and replaced by any qualified service provider.

- FRU – Field-replaceable units must be removed and installed only by authorized Oracle service personnel.

Components also have three service classifications:

- Hot -pluggable – Using the proper software commands, you can install or remove hot-pluggable components while the system is running.

- Hot-swappable – Hot-swappable components can be installed or removed while the system is running, without using any software commands.

- Cold-swappable - You must remove power from the system to service the components.

Component Name | Component Type | Service Classification
--- | --- | ---
Power supply | CRU | Hot-swap
Power supply fan tray | CRU | Hot-swap
Server module | CRU | Hot-plug
Front indicator module (FIM) | CRU | Hot-swap
Chassis monitoring module (CMM) | CRU | Hot-swap
Network express module (NEM) | CRU | Hot-swap, hot-plug, or cold-swap, depending on NEM type
PCIe ExpressModule (PCIe EM) | CRU | Hot-plug
Rear fan module | CRU | Hot-swap
Fan board | CRU | Cold-swap (Power off the chassis)
Midplane | FRU | Cold-swap (Power off the chassis)
Internal power cables | FRU | Cold-swap (Power off the chassis)

##### Related Information

- Replacing Customer-Replaceable Units

- Replacing Field-Replaceable Units

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |