Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Overview

Search Scope:

- This Document
- Entire Library

#### Storage Modules

Storage modules provide additional storage for server modules. There are currently two types of storage modules supported:

- Sun Blade 6000 Disk Module – This storage module is SAS-1 capable and can work with SAS-1 NEMs and a SAS-1 REM installed on a server module.

  In a SAS-1 configuration, a disk module is slot-paired to a server module, with the controlling server module in an even-numbered slot and the disk module installed in the adjacent odd-numbered slot to the right of the controlling server, as viewed from the front of the chassis (for example, 0+1, 2+3).

- Sun Blade Storage Module M2 – This storage module is SAS-2 capable and can work only in a Sun Blade 6000 modular system chassis with a PCIe 2.0 midplane (chassis model A90-B, A90-D, or 7105379) and SAS-2 NEMs installed.

  Controlling server modules must have a SAS-2 REM installed. The storage devices available on this storage module must be assigned to server modules using the Oracle ILOM CMM Sun Blade Zone Manager. Refer to the Oracle ILOM documentation for more information.

The following table lists the blade storage modules and provides the location of the storage module documentation:

Module | Documentation Web Site
--- | ---
Sun Blade 6000 Disk Module | http://docs.oracle.com/cd/E19045-01/index.html
Sun Blade Storage Module M2 | http://download.oracle.com/docs/cd/E19452-01/index.html

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |