Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Site Planning Guide

Search Scope:

- This Document
- Entire Library

#### Power Cords

The connection to the Sun Blade 6000 chassis AC inlet requires the following types of power cords, dependent on site location and power source.

- If you are connecting the system directly to an external power source (for example, power is not obtained through a modular power system), use the power cords described in the following table.

  Location | Oracle Part Number | Quantity | Length | Connections
  --- | --- | --- | --- | ---
  Americas Domestic | X5044A-Z | 4 | 4 meters | NEMA L6-20P to IEC320-C19
  Americas Domestic | X5915A-N1 | 2 | 4 meters | NEMA L6-30P to NEMA L6-20R
  International | X5045A-Z |  | 4 meters | IEC309, 16A, 3 pin to IEC320-C1

  1Requires X5044A-Z. Order Qty 2 X5915-N for each X5044A-Z ordered

- If you are connecting the system to a (rack internal) modular power system, use this type of power cord: IEC320-C19 to IEC320-C20 – 1.5 meter, Oracle part number X5046A-Z; 2.0 meter, Oracle part number X5047A-Z

Copyright © 2008, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |