Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

## Install a NEM

1. Align the NEM with the vacant NEM slot.

   If you are installing only one NEM, it should be installed in the bottom (NEM 0) slot.

2. Ensure that:

   - The RJ-45 port connectors of the NEM are facing you.

   - The NEM ejector levers are fully opened.

   - The NEM ejector levers are on the top of the module.

3. Slide the NEM into the vacant NEM chassis slot until you feel it stop.
4. Close the ejector levers to secure the NEM in the chassis.

##### Related Information

- Remove a NEM

- Monitoring Faults

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |