Skip Navigation Links
Exit Print View
| Oracle Integrated Lights Out Manager (ILOM) 3.x ### Supplement for the Sun Blade 6000 Modular System

Search Scope:

- This Document
- Entire Library

#### Chassis Sensors in Oracle ILOM 3.0

The following tables list the chassis sensors.

Note - For ILOM 3.1, replace `/CH` with `/SYSTEM`.

Sensor | Reading | State | Event | Description
--- | --- | --- | --- | ---
`/CH/HOT` | `0x0001` | State Deasserted | No | Indicates that monitored temperatures do not require full fan speed.
| `0x0002` | State Asserted | No | Indicates that monitored temperatures require increased fan speed.

Sensor | Threshold | Description
--- | --- | ---
`/CH/T_AMB` | Value | Reports ambient temperature in the chassis midplane.
| Upper nonrecoverable |
| Upper critical |
| Upper noncritical |
| Lower noncritical |
| Lower critical |
| Lower nonrecoverable |
`/CH/VPS` | Value | Virtual power sensors that report the total power used by the chassis (the sum of `PS0/IN_POWER` and `PS1/IN_POWER`).
| Upper nonrecoverable |
| Upper critical |
| Upper noncritical |
| Lower noncritical |
| Lower critical |
| Lower nonrecoverable |

##### Related Information

- Display Sensor Readings (CLI)

- Fan Sensors in Oracle ILOM 3.0

- Power Supply Sensors in Oracle ILOM 3.0

- NEM Sensors in Oracle ILOM 3.0

- Server Module Sensors in Oracle ILOM 3.0

- Sensor Types

Copyright © , 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |