Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

## Install the CMM

1. Align the CMM with the CMM slot.

   Ensure that the CMM indicator LEDs of the CMM on the front panel are on the top of the module and facing you.

2. Slide the CMM into the vacant CMM chassis slot.

   Ensure that the CMM engages with the system chassis guidance system.

3. Close the ejector lever to secure the CMM in the chassis.

   After you install a CMM in a powered-on system, the CMM automatically begins to initialize.

##### Related Information

- CMM Reset Sequence

- Remove the CMM

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |