Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

#### Chassis and CMM LEDs

A fault is declared and the chassis Temperature Fail LEDs are illuminated when the external condition represents a potential hazard to the system. An external fault can force a shutdown of the entire system. The chassis Service Action Required LED also lights when there is a fault on a chassis component.

Figure 1 Chassis and CMM LEDs

Figure Legend

1 Locate LED

2 Service Action Required LED

3 Power/OK LED

4 Temperature Fail LED

##### Related Information

- Power Supply LEDs

- Rear Fan LEDs

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |