Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

## Prepare the Chassis for Removal

1. Label and record the locations of all the cables that are connected to the modular system.

   Performing this step ensures that each cable can be returned to its original location.

2. Disconnect all data cables that are connected to components in the chassis.
3. Ensure that no power is applied to the chassis.

   See Power Off the Chassis.

   | Caution - Verify that no voltage is applied to the chassis before you continue.

##### Related Information

- Depopulate the Chassis

- Remove the Chassis From the Rack

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |