Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

## Remove a PCIe EM

Before You Begin

You need to prepare the PCIe EM for removal through the associated server module operating system. If you are hot-plugging the PCIe EM, press the Attention button to prepare the operating system.

1. Verify that the PCIe EM Power LED is off.

   If you have successfully prepared the PCIe EM for a hot-remove, the Power LED goes out.

2. Place one finger on top of the ejector lever handle.
3. Pull the ejector lever toward you to pull the PCIe EM forward until you can pull the rest of the module out by hand.

   | Caution - If you are not immediately replacing the PCIe EM, install a PCIe EM filler panel to ensure proper system operation.

##### Related Information

- Install a PCIe EM

- PCIe EM Service Overview

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |