Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

## Remove a NEM

1. Remove all cables from the NEM.
2. Press together and hold the ejector buttons on both the right and left ejector levers.
3. To unlatch the NEM from the chassis, open the ejector levers by extending them outward.
4. Holding the opened ejector levers, pull the NEM toward you until you can pull the rest of the module out by hand.

   | Caution - If you are not immediately replacing the NEM, install a NEM filler panel to ensure proper system temperature and operation.

##### Related Information

- Install a NEM

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |