Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Site Planning Guide

Search Scope:

- This Document
- Entire Library

### Secure Installation Requirements

To minimize personal injury in the event of a seismic occurrence, you must securely fasten the cabinet in which the system is rackmounted to a rigid structure extending from the floor to the ceiling, or from the walls, of the room in which the cabinet is located.

Install a stand-alone system or a rackmounted system on a level surface. At the base of the cabinet is an anti-tilt bar. This bar must be extended before you install the Sun Blade 6000 modular system to prevent the cabinet from moving.

Copyright © 2008, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |