Skip Navigation Links
Exit Print View
| Oracle Integrated Lights Out Manager (ILOM) 3.x ### Supplement for the Sun Blade 6000 Modular System

Search Scope:

- This Document
- Entire Library

#### NEM Sensors in Oracle ILOM 3.0

The following table lists possible sensors for NEMs (NEM0 and NEM1).

Note - Not all NEMs have all sensors.

Sensor | Reading | State | Event | Description
--- | --- | --- | --- | ---
`NEMn/PRSNT` | `0x0001` | Device Absent | Yes | NEM is absent.
| `0x0002` | Device Present | Yes | NEM is present.
`NEMn/STATE` | `0x0001` | Running | Yes | NEM is running.
| `0x0004` | Powered Off | Yes | NEM is powered off.
| `0x0040` | Degraded | Yes | NEM needs to be serviced.
`NEMn/ERR` | `0x0001` | Predictive Failure Asserted | Yes | NEM has failed.
| `0x0002` | Predictive Failure Deasserted | Yes | NEM has not failed.

##### Related Information

- Sensor Types

- Display Sensor Readings (CLI)

- Chassis Sensors in Oracle ILOM 3.0

- Fan Sensors in Oracle ILOM 3.0

- Power Supply Sensors in Oracle ILOM 3.0

- Server Module Sensors in Oracle ILOM 3.0

Copyright © , 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |