Skip Navigation Links
Exit Print View
| Sun Blade 6000 and Sun Blade 6048 Modular System ### Safety and Compliance Guide Compliance Model No.: 6000/CNST48

Search Scope:

- This Document
- Entire Library

## English

Hardwire connections between systems or systems and peripherals using ports other than modular jack ports must use shielded cables to comply with radio frequency emission limits. Any modular jack serial ports or wired Ethernet port connections may be made using unshielded twisted pair (UTP) cables.

Copyright © 2006, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |