Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Overview

Search Scope:

- This Document
- Entire Library

#### Identifying CMM Models

There are three models of CMM modules available, depending on the chassis that you have. The following illustrations show the layout of the CMM types.

The following illustration shows the CMM module that is supported with the A90-A/B chassis.

The following illustration shows the CMM that is supported with the A90-D and 7105379 chassis. The CMMs for these chassis have different part numbers, but they have the same layout.

Note - For a more detailed description of how to identify which CMM module goes with which chassis, see the Sun Blade 6000 Modular System Service Manual.

Legend Table
1 | SER MGT port
2 | NET MGT 0 port

Note - The A90-B chassis might have the NET MGT 0 port covered. This can be removed if you want to use the NET MGT port 1. Refer to the Oracle ILOM CMM Administration Guide for the Sun Blade 6000 Modular System for instructions on enabling the NET MGT port 1.

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |