Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

## Remove the CMM

1. Remove any cables connected to the CMM.
2. Press together and hold the ejector button on the module ejector lever.To unlatch the module from the chassis, pull the ejector lever away from the module and up.
3. Pull the ejector lever toward you until you are able to pull the rest of the module out by hand.

   | Caution - To ensure proper system cooling and operation, you must replace the CMM within one minute or you must power off the chassis.

##### Related Information

- Install the CMM

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |