Index

### Numerics

7-Segment Display

diagnostic codes, 1

expansion tray codes, 1

### A

array

powering-off, 1

power-on procedures, 1

pre-installation process for, 1

### B

Battery Fault LED, 1

bootstrap protocol (BOOTP) services, 1

### C

cabling

data hosts, 1

direct topology, 1

Ethernet crossover cable, 1

FC switch topology, 1

for out-of-band management, 1

in-band management connection, 1

power connections, 1

Cache Active LED, 1

cache memory DIMM failure detected, 1

Configuration wizard for DHCP, 1

controller modules

CRUs, 1

FC LEDs, 1

Service Action Required, 1

controller trays

7-Segment Display, 1

diagnostic sequences, 1

front-access components, 1

LEDs on the rear, 1

rear-access components, 1

sequence code definitions, 1

SFP transceivers, 1

CRUs

controller module, 1

disk drives, 1

input/output modules (IOMs), 1

power-fan module, 1

Service Advisor replacement procedures, 1

### D

data host

cabling, 1

multipathing software, 1

DC power option, 1

DHCP

Configuration wizard for, 1

server configuration, 1

Solaris DHCP server setup, 1

diagnostic code sequences, 1

diagnostic LEDs, 1

direct topology

cabling, 1

disk drives

LEDs, 1

maximum support, 1

numbering scheme, 1

tray ID and slot designation, 1

drive expansion trays

front-access components, 1

I/O module, 1

overview, 1

rear-access components, 1, 2

### E

Ethernet crossover cable, 1

Ethernet ports, 1, 2

expansion trays

7-Segment Display, 1

components, 1

connecting IOM ports, 1

Ethernet port, 1

I/O module, 1

IOMs, 1

power-fan modules, 1

### F

fans, power-fan module, 1

fault LED, 1

FC disk drives, 1

FC switch topology

cabling, 1

Fibre Channel host ports, 1

flash drive failure detected, 1

### H

HBAs

host card failure, 1

host port WWN, 1

in-band management cabliing, 1

host card failure detected, 1

host ports

Fibre Channel, 1

SAS-2, 1

### I

in-band management

cabling, 1

proxy agent, 1

installation process, 1

IOMs

communication loss, 1

expansion tray, 1

Fibre Channel interface failure, 1

hot swap, 1

replacement procedures, 1

### L

LEDs

diagnostic, 1

fault, 1

Locate, 1

on the rear of the trays, 1

power-fan module, 1

Service Action Allowed, 1, 2

Service Action Required, 1

lockdown condition detected, 1

### M

MAC address location, 1

management host software, installing, 1

multipathing software, viii, 1

### O

out-of-band management

cabling, 1

Ethernet connection example, 1

IP addressing, 1

over-temperature condition, 1

### P

persistent memory error, 1

power

connecting cables, 1

DC option, 1

Power LED, 1

power-fan module

CRUs, 1

description of, 1

fan, description of, 1

LEDs, 1

powering off the array, 1

power-on procedures, 1

processor DIMM failure detected, 1

product overview

software, 1

### R

RAID Proxy Agent, 1

rear-access components of the drive expansion tray, 1

redundancy

connecting controller to expansion trays, 1

fibre channel example, 1

host cabling, 1

I/O module, 1

### S

SAS-2 disk drives, 1

SAS-2 host ports, 1

Service Action Allowed LED, 1, 2

Service Action Required LED, 1

Service Advisor, 1

IOM replacement procedures, 1

SFP transceivers

connecting, 1

description of, 1

speed mismatch, 1

standard in ship kit, 1

software overview, 1

Standby Power LED, 1

### T

tray ID

7-Segment display, 1

controller tray diagnostic codes, 1

disk drives, 1

trays

controller, 1

expansion, 1

front-access components, 1

LEDs on the rear, 1

### W

Windows 2000 Advanced Server DHCP requirements, 1

Windows 2000 Advanced Server installation, 1

Copyright © 2011, Oracle and/or its affiliates. All rights reserved.