Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### DIMM FRU Names

DIMM FRU IDs are based on their corresponding location on the motherboard, and are identified using the following convention:

`/SYS/MB/CMP0/BOBx/CHx/Dx`

Specific DIMM FRU IDs are described in the following illustration.

Figure 42 DIMM Slot FRU IDs

Figure Legend

1 For a 1/4-full configuration, populate only the slot locations labeled 1.

2 For a 1/2-full configuration, populate the slot locations labeled 1 and 2.

3 For a fully populated configuration, fill all the DIMM slots.

##### Related Information

- DIMM Population Rules

- Supported DIMM Configurations

- DIMM Rank Classification Labels

- Increase System Memory With Additional DIMMs

- Verify DIMM Functionality

- DIMM Configuration Error Messages

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |