Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Stabilize the Rack

| Caution - To reduce the risk of personal injury, stabilize the expansion rack cabinet and extend all anti-tilt devices before installing the server.

Refer to your rack documentation for detailed instructions for the following steps.

1. Open and remove the front and rear doors from the rack cabinet.
2. To prevent the rack cabinet from tipping during the installation, stabilize the cabinet using all anti-tilt mechanisms provided.
3. If there are leveling feet beneath the rack cabinet to prevent it from rolling, extend these leveling feet fully downward to the floor.
4. Fully extend the rack cabinet's anti-tilt legs or anti-tilt bar, which are located at the bottom front of the rack cabinet.

##### Related Information

- The rack documentation

- SPARC T4-1 Server Safety and Compliance Guide

- Rack Compatibility

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |