Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

### Installing the Server

These topics describe how to install the server into a rack using the rail assembly in the rackmount kit. Perform these procedures if you purchased the rail assembly.

Note - In this guide, the term rack means either an open rack or a closed cabinet.

Step | Description | Links
--- | --- | ---
1. | Verify that the rack is compatible with the server's installation requirements. | Rack Compatibility
2. | Take antitilt precautions to ensure the rack does not tip forward when the server is installed. | Stabilize the Rack
3. | Attach the slide rails. | Install the Slide Rail Assemblies
4. | Install the server in the rack. | Install the Server
5. | (Optional) Install the CMA. | Install the CMA
6. | Verify that the slide rails and CMA (if used) operate correctly. | Verify Correct Operation of the Slide Rails and the CMA

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |