Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### Video Port

The server has one 15-pin VGA video port located on the server's rear panel. Maximum supported resolution is 1024 x 768.

Figure 24 Video Connector

Figure Legend

1 Red Video

2 Green Video

3 Blue Video

4 Monitor ID - Bit 2 (Ground)

5 Ground

6 Red Ground

7 Green Ground

8 Blue Ground

9 +5V

10 Sync Ground

11 Monitor ID - Bit 0 (Ground)

12 VGA 12C Serial Data

13 Horizontal Sync

14 Vertical Sync

15 VGA 12C Serial Clock

##### Related Information

- Rear Panel Components

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |