Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Release the CMA

For some service procedures, if you are using a CMA, you might need to release it to gain access to the rear of the chassis.

Note - For instructions on how to install the CMA for the first time, refer to your server Installation Guide.

- Complete the following tasks to release the CMA:
  1. Press and hold the tab (step A).
  2. Swing the CMA out of the way (step B).

     When you have finished with the service procedure, swing the CMA closed and latch it to the left rack rail.

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |