Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Reinstall the Server in the Rack

| Caution - The chassis is heavy. To avoid personal injury, use two people to lift it and set it in the rack.

1. Place the ends of the chassis mounting brackets into the slide rails.
2. Slide the server into the rack until the brackets lock into place.

   The server is now in the extended maintenance position.

##### Related Information

- Return the Server to the Normal Rack Position

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |