Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### Automatic System Recovery Overview

The server provides for ASR from failures in memory modules or PCI cards.

ASR functionality enables the server to resume operation after experiencing certain nonfatal hardware faults or failures. When ASR is enabled, the system's firmware diagnostics automatically detect failed hardware components. An autoconfiguring capability designed into the system firmware enables the system to unconfigure failed components and to restore server operation. As long as the server is capable of operating without the failed component, the ASR features enable the server to reboot automatically, without operator intervention.

Note - ASR is not activated until you enable it. See Enable ASR.

For more information about ASR, refer to the service manual for your server.

##### Related Information

- Enable ASR

- Disable ASR

- View Information on Components Affected by ASR

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |