Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### NET MGT Port

The NET MGT RJ-45 port, located on the rear panel, provides an optional Ethernet connection to the service processor.

Figure 22 NET MGT Port

Figure Legend

1 Transmit Data +

2 Transmit Data –

3 Receive Data +

4 No Connect

5 No Connect

6 Receive Data –

7 No Connect

8 No Connect

##### Related Information

- Front Panel Components

- Rear Panel Components

- Connect the NET MGT Port Cable

- Assign a Static IP Address to the SP

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |