Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Install a PCIe or XAUI Card

Note - This is a cold service procedure that can be performed by customers. See Cold Service, Replaceable by Customer for more information about cold service procedures.

| Caution - This procedure involves handling circuit boards that are extremely sensitive to static electricity. Ensure that you follow ESD preventative practices to avoid damaging the circuit boards.

| Caution - Components inside the chassis might be hot. Use caution when servicing components inside the chassis.

1. Perform the preliminary steps required for cold service procedures.

   See Cold Service, Replaceable by Customer for instructions.

2. Locate the proper PCIe/XAUI slot for the card you are replacing.
3. Remove the PCIe/XAUI riser.

   See Remove a PCIe or PCIe/XAUI Riser.

4. If a PCIe filler panel is installed, remove it.
5. Install the PCIe or XAUI card into the riser.

   Before inserting the card, you must rotate the retention clip out of the way, as shown in panel 1.

6. Rotate the retention clip downward and press it until it is securely in place.
7. Reinstall the PCIe/XAUI riser.

   See Install a PCIe or PCIe/XAUI Riser.

8. Connect any data cables required to the PCIe/XAUI card.

   Route data cables through the cable management arm.

##### Related Information

- Remove a PCIe or XAUI Card

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |