Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Install the Connector Board

Note - This is a cold service procedure that must be performed by qualified service personnel. See Cold Service, Replaceable by Authorized Service Personnel for more information about this category of service procedures.

| Caution - The server must be fully shut down and the power cords disconnected.

| Caution - This procedure involves handling circuit boards that are extremely sensitive to static electricity. Ensure that you follow ESD preventative practices to avoid damaging the circuit boards.

| Caution - Components inside the chassis might be hot. Use caution when servicing components inside the chassis.

1. Using the mushroom standoff as an alignment guide, lower the connector board into the chassis.
2. Slide the connector board forward to plug it into the hard drive backplane.
3. Secure the connector board with two screws.
4. Connect the power and data cables from the fan power board.
5. Install the power distribution board.

   See Install the Power Distribution Board.

6. Install the motherboard assembly.

   See Install the Motherboard Assembly.

##### Related Information

- Remove the Connector Board

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |