Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Install the CMA

| Caution - Support the CMA during this installation. Do not allow the assembly to hang by its own weight until it is secured by all three attachment points.

1. Remove the tape from the CMA rail extension (on the left of the CMA) and remove the CMA rail extension.
2. Attach the CMA rail extension to rear left slide rail.

   At the rear of the rack, plug the CMA rail extension into the end of the left sliding rail assembly. The tab at the front of the rail extension clicks into place.

   Figure 14 Inserting the CMA Rail Extension Into the Rear of the Left Slide Rail

   The right sides of the two CMA arms have hinged extensions. On the manufacturer's instruction sheet, the smaller extension is called the CMA Connector for Inner Member. This extension attaches to the right mounting bracket. The larger extension is called the CMA Connector for Outer Member, and attaches to the right sliding rail.

3. Insert the smaller extension into the clip located at the end of the mounting bracket.

   Slide the smaller extension into the square hole on the middle-in-width of the clip that is located at the end of the mounting bracket.

   Figure 15 Mounting the Inner CMA Connector

4. Insert the larger extension into the end of the right sliding rail.

   Figure 16 Attaching the Outer CMA Connector

5. Insert the hinged plastic connector at the left side of the CMA fully into the CMA rail extension.

   The plastic tab on the CMA rail extension locks the hinged plastic connector in place.

   Figure 17 Mounting the Left Side of the Slide Rail

##### Related Information

- Rack Compatibility

- Slide Rail Assemblies

- Install the Slide Rail Assemblies

- Install the Server

- Verify Correct Operation of the Slide Rails and the CMA

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |