Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Install the Server

| Caution - The weight of the servers on extended slide rails can be enough to overturn an equipment rack.

| Caution - The server weighs approximately 60 lb (25 kg). Two people are required to lift and mount the server into a rack enclosure.

1. If the rack is equipped with an antitilt bar, verify that it has been deployed and, if not, deploy it.
2. Insert the ends of the mounting brackets into the sliding rails.

   Figure 13 Mounting the Chassis on the Slide Rails

3. While pressing the two green slide rail release buttons, push the server into the rack until the slide rail locks on the front of the mounting brackets engage the slide rail assemblies. You will hear a click at that point.

   | Caution - Before continuing, verify that the server is securely mounted in the rack, and that the slide rails are locked to the mounting brackets.

##### Related Information

- Rack Compatibility

- Slide Rail Assemblies

- Install the Slide Rail Assemblies

- Install the CMA

- Verify Correct Operation of the Slide Rails and the CMA

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |