Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Remove the System Configuration PROM

Note - This is a cold service procedure that must be performed by qualified service personnel. See Cold Service, Replaceable by Authorized Service Personnel for more information about this category of service procedures.

| Caution - The server must be fully shut down and the power cords disconnected.

| Caution - This procedure involves handling circuit boards that are extremely sensitive to static electricity. Ensure that you follow ESD preventative practices to avoid damaging the circuit boards.

| Caution - Components inside the chassis might be hot. Use caution when servicing components inside the chassis.

Note - The System Configuration PROM is plugged into a socket on the motherboard. It includes a yellow barcode label.

1. Perform the preliminary steps required for cold service procedures.

   See Cold Service, Replaceable by Customer for instructions.

2. Extend the server out of the rack.

   See Extend the Server.

3. If you can access the rear area of the server without removing the server from the rack, go to Step 4, otherwise remove the server from the rack:
   - Unplug all cables from the server.
   - Remove the Server From the Rack
4. Remove the top cover.

   See Remove the Top Cover.

5. Pull up on the System Configuration PROM to remove it from its socket.

   The System Configuration PROM has a yellow barcode label on it.

##### Related Information

- Install the System Configuration PROM

- Verify the System Configuration PROM

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |