Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Remove or Install a Power Supply Filler Panel

This procedure describes how to remove or install a power supply filler panel.

Note - During operation, and empty power supply bay must have a filler panel installed for proper environmental control.

- Depending on your desired task, perform one of the following tasks:

  - Remove a filler panel – Grasp an inside edge of the filler panel and pull out the filler panel.

  - Install a filler panel – Align the filler panel with the empty power supply bay and push it into the bay.

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |