Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### DIMM Configuration Errors—`show faulty` Command Output

In addition to general hardware errors, the `show faulty` command also detects DIMM configuration errors. For example:

    -> show faulty
    Target              | Property               | Value--------------------+------------------------+--------------------------------/SP/faultmgmt/0     | fru                    | /SYS/MB/CMP0/BOB0/CH0/D0/SP/faultmgmt/0/    | class                  | fault.component.misconfigured faults/0           |                        |/SP/faultmgmt/0/    | sunw-msg-id            | SPT-8000-PX faults/0           |                        |/SP/faultmgmt/0/    | component              | /SYS/MB/CMP0/BOB0/CH0/D0 faults/0           |                        |/SP/faultmgmt/0/    | uuid                   | 2caf416b-4fe0-6509-db02-aa719f5d faults/0           |                        | d543/SP/faultmgmt/0/    | timestamp              | 2012-09-24/17:00:40 faults/0           |                        |/SP/faultmgmt/0/    | fru_part_number        | 000-0000 faults/0           |                        |/SP/faultmgmt/0/    | fru_serial_number      | 00CE011217213B151F faults/0           |                        |/SP/faultmgmt/0/    | product_serial_number  | 1140BDY90A faults/0           |                        |/SP/faultmgmt/0/    | chassis_serial_number  | 1140BDY90A faults/0           |                        |

##### Related Information

- DIMM Configuration Errors—System Console

- DIMM Configuration Errors—`fmadm` `faulty` Output

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |