Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Secure Cables in the CMA

1. Once the server cables are connected and placed inside the CMA, open the velcro cable straps and wrap the straps around the CMA securing the cables inside the CMA.

   Figure 29 Securing the Server Cables With the CMA and Velcro Straps

2. Verify the operation of the slide rails and CMA, and cable service loops.

   Repeat the steps described in the procedure: Verify Correct Operation of the Slide Rails and the CMA.

##### Related Information

- Install the CMA

- Verify Correct Operation of the Slide Rails and the CMA

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |