Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Connect the SER MGT Port Cable

The SER MGT port is the farthest left RJ-45 port on the rear panel.

- Connect a Category 5 cable from the SER MGT port to the terminal device.

  Figure 25 SER MGT port – Rear Panel

  This port is needed to set up the NET MGT port.

  When connecting a DB-9 cable, use an RJ-45 to DB-9 adapter to perform the crossovers given for each connector.

  Note - Use the SER MGT port only for server management. This port is the default connection between the SP and a terminal or a computer.

  | Caution - Do not attach a modem to this port.

##### Related Information

- Connect the NET MGT Port Cable

- Connecting Cables

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |