Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

#### Fan Module LEDs

The status of each fan module is displayed by a bi-color LED. These six status LEDs are located on the chassis frame to the right of the fan module bay. The LEDs are labeled with numbers that correspond to fan module labels on the midwall. When the fault manager reports a failed fan module, use the status LEDs to learn the number of the faulty fan module and use the fan locating label on the midwall to identify the fan module.

Figure 49 Fan Module LEDs

Table 33 Fan Module Status LEDs

LED |  | Notes
--- | --- | ---
Fan OK Status (green) |  | The LED is green when the corresponding fan is operational.
Service Required Status (amber) |  | The LED is amber when the fan module is faulty. A faulty fan module will also cause the system Fan Fault LED to be lighted.

When a fan module fault is detected, the front and rear panel Service Required LEDs also turn on.

If the fan fault produces an over temperature condition, the system Overtemp LED will turn on and an error message will be logged and displayed on the system console.

##### Related Information

- Fan Configuration Reference

- Locate a Faulty Fan Module

- Remove a Fan Module

- Install a Fan Module

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |