Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Connect the NET MGT Port Cable

Before You Begin

The NET MGT port is located just to the right of the SER MGT port on the rear panel.

- Connect a Category 5 cable from the NET MGT port to your network switch or hub.

  Figure 26 NET MGT port – Rear Panel

  Note - This port is not operational until you configure the network settings (through the SER MGT port).

  Note - The NET MGT port is configured by default to retrieve network settings with Dynamic Host Configuration Protocol (DHCP) and allow connections using SSH. You might need to modify these settings for your network. Instructions are given in Powering On the Server for the First Time.

##### Related Information

- Connect the SER MGT Port Cable

- Connecting Cables

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |