Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### Gigabit Ethernet Ports

Four RJ-45 Gigabit-Ethernet connectors (NET0, NET1, NET2, NET3) are located on the rear panel. The Ethernet interfaces operate at 10 Mbit/sec, 100 Mbit/sec, and 1000 Mbit/sec.

Figure 23 Gigabit Ethernet Port

Figure Legend

1 Transmit/Receive Data 0 +

2 Transmit/Receive Data 0 –

3 Transmit/Receive Data 1 +

4 Transmit/Receive Data 2 +

5 Transmit/Receive Data 2 –

6 Transmit/Receive Data 1 –

7 Transmit/Receive Data 3 +

8 Transmit/Receive Data 3 –

##### Related Information

- Front Panel Components

- Rear Panel Components

- Connect the NET MGT Port Cable

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |