Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

#### PCIe Card Configuration Reference

Use the following table to plan your PCIe/XAUI card configuration on SPARC T4-1 server.

Table 32 PCIe and XAUI Support

Slot | PCIe Switch | Supported Device Types | FRU Name
--- | --- | --- | ---
PCIe 0 or XAUI 01 | 0 | PCIe (x16 physical, x8 electrical) XAUI expansion card | `/SYS/MB/RISER0/PCIE0` `/SYS/MB/RISER0/XAUI0`
PCIe 1 | 1 | PCIe (x16 physical, x8 electrical) | `/SYS/MB/RISER1/PCIE1`
PCIe 2 | 0 | PCIe (x16 physical, x8 electrical) | `/SYS/MB/RISER2/PCIE2`
PCIe 3 or XAUI 1 | 1 | PCIe (x8 physical, x8 electrical) XAUI expansion card | `/SYS/MB/RISER0/PCIE3` `/SYS/MB/RISER0/XAUI1`
PCIe 4 | 0 | PCIe (x8 physical, x8 electrical) | `/SYS/MB/RISER1/PCIE4`
PCIe 5 | 1 | PCIe (x8 physical, x8 electrical) | `/SYS/MB/RISER2/PCIE5`

1Slots 0 and 3 are capable of accepting either PCIe or XAUI cards. You can only install one type of card.

Note - As a general rule, the PCIe and PCIe/XAUI slots should be populated sequentially, beginning with slot 0 and progressing to slot 5. This general rule does not apply to I/O cards that have special slot restrictions. For guidance on these restrictions, see the table, PCIe Slot Usage Rules for Certain HBA Cards in the SPARC T4-1 Server Product Notes.

##### Related Information

- Remove a PCIe or XAUI Card

- Install a PCIe or XAUI Card

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |