Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Install the Front Panel Light Pipe Assembly (Right or Left)

Note - This is a cold service procedure that must be performed by qualified service personnel. See Cold Service, Replaceable by Authorized Service Personnel for more information about this category of service procedures.

| Caution - The server must be fully shut down and the power cords disconnected.

| Caution - This procedure involves handling circuit boards that are extremely sensitive to static electricity. Ensure that you follow ESD preventative practices to avoid damaging the circuit boards.

| Caution - Components inside the chassis might be hot. Use caution when servicing components inside the chassis.

Note - The following steps apply to both right and left light pipe assemblies.

1. Align the individual light pipes with the corresponding holes in the front panel flange.
2. Lay the light pipe assembly on the metal mounting plate with its attachment hooks inserted into the corresponding holes in the plate.

   Note - The two locator pins will not line up with their holes until the next step.

3. Slide the assembly forward until the attachment hooks and locator pins are fully engaged.

   Tip - Verify that the tip of each light pipe is flush with the front surface of the flange. This is a sign that the assembly is properly installed on the mounting plate.

4. Align the screw holes in the metal mounting plate with the holes on the side of the hard drive cage.
5. Secure the light pipe assembly with the three screws.
6. Install the hard drive cage.

   See Install the Hard Drive Cage.

##### Related Information

- Remove the Front Panel Light Pipe Assembly (Right or Left)

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |